{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["数量清单"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"数量清单","index":0,"n_rows":15,"n_cols":8,"rows_kept":15,"merged":[[0,0,0,7],[1,0,1,7],[17,1,17,7],[18,1,18,7],[19,1,19,7]]}
["150米三峡游轮复合岩棉板数量清单"]
["船名：重轮长江云帆             工程编号：ZJ20-LYC007"]
["序号","产品名称","产品规格","单位","数量","单价","总价","备注"]
[1,"A型复合岩棉壁板","t=50mm，两侧面板0.6mm镀锌钢板裸板，芯材岩棉，溶重120kg/m³，其中两张内部按照电视机规格加强","㎡",1523.5]
[2,"A型复合岩棉壁板","t=50mm，两侧面板0.6mm镀锌钢板贴PVC，芯材岩棉，溶重120kg/m³","㎡",1664.9,null,null,"浅木纹色"]
[3,"A型单面贴塑衬板","t=25mm，面板0.6mm钢板贴塑，背板0.6mm镀锌钢板，芯材岩棉，溶重120kg/m³","㎡",14321,null,null,"浅木纹色"]
[4,"A型单面贴塑衬板","t=25mm，面板0.6mm钢板贴塑，背板0.6mm镀锌钢板，芯材岩棉，溶重120kg/m³","㎡",728.6,null,null,"深木纹色"]
[5,"A型单面贴塑衬板","t=25mm，面板0.6mm钢板贴塑，背板0.6mm镀锌钢板，芯材岩棉，溶重120kg/m³","㎡",2299.1,null,null,"米色"]
[6,"A型复合岩棉壁板带暗铰链天地销锁检修门","t=50mm，两侧面板0.6mm镀锌钢板贴PVC，芯材岩棉，溶重120kg/m³","个",194,null,null,"浅木纹色\n开孔1600×400"]
[7,"A型单面贴塑衬板直角转角","t=25mm，面板0.6mm钢板贴塑，背板0.6mm镀锌钢板，芯材岩棉，溶重120kg/m³","㎡",196.6,null,null,"米色规格L=120*120/H=2.38"]
[8,"A型单面贴塑衬板直角转角带灯槽","t=25*35mm，面板0.6mm钢板贴塑，背板0.6mm镀锌钢板，芯材岩棉，溶重120kg/m³","㎡",174.1,null,null,"浅木纹色规格L=165*100/H=2.38"]
[9,"A型单面贴塑衬板直角转角","t=25mm，面板0.6mm钢板贴塑，背板0.6mm镀锌钢板，芯材岩棉，溶重120kg/m³","㎡",174.1,null,null,"浅木纹色，规格L=165*100/H=2.38"]
[10,"A型单面贴塑衬板内圆转角","t=25mm，面板0.6mm钢板贴塑，背板0.6mm镀锌钢板，芯材岩棉，溶重120kg/m³","㎡",1576.5,null,null,"浅木纹色，规格L=490*280/H=2.38/R100"]
[11,"A型单面贴塑衬板内圆转角带灯槽","t=25mm，面板0.6mm钢板贴塑，背板0.6mm镀锌钢板，芯材岩棉，溶重120kg/m³","㎡",525.5,null,null,"浅木纹色，规格L=490*280/H=2.38/R100"]
[12,"A型单面贴塑衬板","t=25mm，面板0.6mm不锈钢板，背板0.6mm镀锌钢板，芯材岩棉，溶重120kg/m³","㎡",1649,null,null,"不锈钢板"]